11/11/2020
20:15:35
Created by Short Cut (4.3)
Short Cut Program:  measure-13tc.DEF

-Wiring for CR10-

  AM25T
    1H:  HI
    1L:  LO
    AG:  Ground
    E1:  VX
    C2:  RES
    C1:  CLK
    G:  G
    12V:  12V

-Wiring for AM25T-

  Type K TC (1)
    1H:  Yellow
    1L:  Red

  Type K TC (2)
    2H:  Yellow
    2L:  Red

  Type K TC (3)
    3H:  Yellow
    3L:  Red

  Type K TC (4)
    4H:  Yellow
    4L:  Red

  Type K TC (5)
    5H:  Yellow
    5L:  Red

  Type K TC (6)
    6H:  Yellow
    6L:  Red

  Type K TC (7)
    7H:  Yellow
    7L:  Red

  Type K TC (8)
    8H:  Yellow
    8L:  Red

  Type K TC (9)
    9H:  Yellow
    9L:  Red

  Type K TC (10)
    10H:  Yellow
    10L:  Red

  Type K TC (11)
    11H:  Yellow
    11L:  Red

  Type K TC (12)
    12H:  Yellow
    12L:  Red

  Type K TC (13)
    13H:  Yellow
    13L:  Red

-Measurement Labels-

  Default
    1  BattV
    2  ProgSig

  AM25T
    3  RTemp_C

  Type K TC (1)
    4  Temp_C_0

  Type K TC (2)
    5  Temp_C_1

  Type K TC (3)
    6  Temp_C_2

  Type K TC (4)
    7  Temp_C_3

  Type K TC (5)
    8  Temp_C_4

  Type K TC (6)
    9  Temp_C_5

  Type K TC (7)
    10  Temp_C_6

  Type K TC (8)
    11  Temp_C_7

  Type K TC (9)
    12  Temp_C_8

  Type K TC (10)
    13  Temp_C_9

  Type K TC (11)
    14  Temp_C_10

  Type K TC (12)
    15  Temp_C_11

  Type K TC (13)
    16  Temp_C_12

Estimated final storage locations used per day:       0
