
-----------------------------------
       Cantera C++ examples        
-----------------------------------




>>>>>  example 1

Description:  
Ignition simulation using class IdealGasMix with file gri30.cti.
Constant-pressure ignition of a hydrogen/oxygen/nitrogen mixture 
beginning at T = 1001 K and P = 1 atm.
 Tfinal = 2663.78
Output files:
  kin1.csv    (Excel CSV file)
  kin1.dat    (Tecplot data file)




>>>>>  example 2

Description:  
Ignition simulation using class IdealGasMix with file gri30.cti.
Constant-pressure ignition of a hydrogen/oxygen/nitrogen mixture 
beginning at T = 1001 K and P = 1 atm.
 Tfinal = 2663.78
Output files:
  kin3.csv    (Excel CSV file)
  kin3.dat    (Tecplot data file)




>>>>>  example 3

Description:  
Chemical equilibrium.
Equilibrium composition and pressure for a range of temperatures at constant density.


**** WARNING ****
For species SI2H6, discontinuity in h/RT detected at Tmid = 1000
	Value computed using low-temperature polynomial:  19.8328
	Value computed using high-temperature polynomial: 19.9055


**** WARNING ****
For species SI2H6, discontinuity in s/R detected at Tmid = 1000
	Value computed using low-temperature polynomial:  49.5493
	Value computed using high-temperature polynomial: 49.7214


**** WARNING ****
For species SI3H8, discontinuity in h/RT detected at Tmid = 1000
	Value computed using low-temperature polynomial:  29.3028
	Value computed using high-temperature polynomial: 29.4297


**** WARNING ****
For species SI3H8, discontinuity in s/R detected at Tmid = 1000
	Value computed using low-temperature polynomial:  65.9731
	Value computed using high-temperature polynomial: 66.2781


**** WARNING ****
For species SI2, discontinuity in h/RT detected at Tmid = 1000
	Value computed using low-temperature polynomial:  74.0115
	Value computed using high-temperature polynomial: 74.0387


**** WARNING ****
For species SI2, discontinuity in s/R detected at Tmid = 1000
	Value computed using low-temperature polynomial:  32.8813
	Value computed using high-temperature polynomial: 32.9489
Output files:
  eq1.csv    (Excel CSV file)
  eq1.dat    (Tecplot data file)




>>>>>  example 5

Description:  
Mixture-averaged transport properties.
Viscosity, thermal conductivity, and mixture-averaged
diffusion coefficients at 2 atm for a range of temperatures
Output files:
  tr1.csv    (Excel CSV file)
  tr1.dat    (Tecplot data file)




>>>>>  example 6

Description:  
Multicomponent transport properties.
Viscosity, thermal conductivity, and thermal diffusion
 coefficients at 2 atm for a range of temperatures
Output files:
  tr2.csv    (Excel CSV file)
  tr2.dat    (Tecplot data file)
