/*--------------------------------*- C++ -*----------------------------------*\
| =========                 |                                                 |
| \\      /  F ield         | OpenFOAM: The Open Source CFD Toolbox           |
|  \\    /   O peration     | Version:  1.7.1                                 |
|   \\  /    A nd           | Web:      www.OpenFOAM.com                      |
|    \\/     M anipulation  |                                                 |
\*---------------------------------------------------------------------------*/
FoamFile
{
    version     2.0;
    format      binary;
    class       dictionary;
    location    "constant";
    object      CMCdict;
}
// * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * //

init_start_CMC true;

latestCMCresultsFileName CMCresults.0.dat;

CMCresults_Time "1.23";//CMC results time for restart

previousnf 1; // number of previous flame group

multipleFG true;

nf 4; //number of flame group to inject

fuelperFG 1e-9; //Inject new FG when mass of injected fuel is greater than fuelperFG

SLFMinit_FileName sdr10.inp;//SLFM libray for initial profile of new flame group

fuel_name CH4;//Main fuel name

//eta-space division 
uni_eta false;

section 4;//Divide eta-space 

etamax 75; //Total number of eta point
          
non_uni_eta_dict
{       
        MFcut (0.0 0.27 0.54 0.77 1.0);//Eta section point
        Neta (0 25 50 65 75); //The number of eta point in each eta section
}


// ************************************************************************* //
