/*--------------------------------*- C++ -*----------------------------------*\
| =========                 |                                                 |
| \\      /  F ield         | OpenFOAM: The Open Source CFD Toolbox           |
|  \\    /   O peration     | Version:  1.7.1                                 |
|   \\  /    A nd           | Web:      www.OpenFOAM.com                      |
|    \\/     M anipulation  |                                                 |
\*---------------------------------------------------------------------------*/
FoamFile
{
    version     2.0;
    format      binary;
    class       dictionary;
    location    "constant";
    object      sprayProperties;
}
// * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * //

interpolationSchemes
{
    U               cellPointFace;
    rho             cell;
    p               cell;
    T               cell;
}

subCycles       2;

Gasjet off;

Cent 0.0247;

atomizationModel blobsSheetAtomization;
//atomizationModel LISA;
//atomizationModel	off;

includeOscillation yes;

breakupModel    ReitzKHRT;

injectorModel   hollowConeInjector;

collisionModel  trajectory;
//collisionModel	off;

evaporationModel standardEvaporationModel;

heatTransferModel RanzMarshall;

dispersionModel stochasticDispersionRAS;
//dispersionModel 	off;

dragModel       standardDragModel;

wallModel       reflect;

sprayIteration
{
    sprayIterate 1;
    sprayRelaxFactor 1;
    minimumParcelMass 1e-20;
}

specConstAtomizationCoeffs
{
    dropletNozzleDiameterRatio ( 0.4 );
    sprayAngle      ( 10 );
}

LISACoeffs
{
	Cl	0.5;
	cTau	12.0;
	Q	1.0e-3;
	J	0;
}

trajectoryCoeffs
{
	cSpace	1;
	cTime	0.3;
	coalescence	on;
}

blobsSheetAtomizationCoeffs
{
	B	1.0;
	angle	30.0;
}

TABCoeffs
{
    y0              0;
    yDot0           0;
    Cmu             10;
    Comega          8;
    WeCrit          12;
}

ETABCoeffs
{
    Cmu             10;
    Comega          8;
    WeCrit          12;
    k1              0.2;
    k2              0.2;
    WeTransition    100;
}

ReitzDiwakarCoeffs
{
    Cbag            6;
    Cb              0.785;
    Cstrip          0.5;
    Cs              10;
}

ReitzKHRTCoeffs
{
    B0              0.61;
    B1              40;  //40
    Ctau            1;
    CRT             0.1;
    msLimit         0.2;
    WeberLimit      6;
}

trajectoryCoeffs
{
    cSpace          1;
    cTime           0.3;
}

standardDragModelCoeffs
{
    preReFactor     0.166667;
    ReExponent      0.666667;
    ReLimiter       1000;
    CdLimiter       0.44;
    Cdistort        2.632;
}

standardEvaporationModelCoeffs
{
    evaporationScheme explicit;
    preReScFactor   0.6;
    ReExponent      0.5;
    ScExponent      0.333333;
}

RanzMarshallCoeffs
{
    preRePrFactor   0.6;
    ReExponent      0.5;
    PrExponent      0.333333;
}

hollowConeInjectorCoeffs
{
    dropletPDF
    {
        pdfType         RosinRammler;
        RosinRammlerPDF
        {
            minValue        100e-06;
            maxValue        200e-06;
            d               135e-6;
            n               3;
        }

        exponentialPDF
        {
            minValue        0.0001;
            maxValue        0.001;
            lambda          10000;
        }
    }

    innerConeAngle  ( 0 );
    outerConeAngle  ( 13 );
}

reflectCoeffs
{
    elasticity      0.9;
}


// ************************************************************************* //
