/*--------------------------------*- C++ -*----------------------------------*\
| =========                 |                                                 |
| \\      /  F ield         | OpenFOAM: The Open Source CFD Toolbox           |
|  \\    /   O peration     | Version:  2.3.0                                 |
|   \\  /    A nd           | Web:      www.OpenFOAM.org                      |
|    \\/     M anipulation  |                                                 |
\*---------------------------------------------------------------------------*/
FoamFile
{
    version     2.0;
    format      ascii;
    class       dictionary;
    location    "constant";
    object      combustionProperties;
}
// * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * //
postSpeciesN 2; //number of species for post-processing
stoiMF 0.351; //stoichiometric mixture fraction
stretchFactor 1.05;
lowerN 20; //number of eta-space under stoichiometric value
upperN 30; //number of eta-space over stoichiometric value

Equilibrium true;
NVar 40; //20;

Sc 0.68; //Schmidt number
outletName outlet; // outletName

detailedEta
(
1e-6 1e-5 1e-4 1e-3 1e-2 
0.1 0.9 
0.99 0.999 0.9999 0.99999 0.999999
);

detailedN
(
10 10 10 10 10
100
10 10 10 10 10
);

NstFolder slfm_lib; //folder name of SLFM library
NstList //list of Nst
(
1
);

// * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * //
