

**** WARNING ****
For species SI2H6, discontinuity in h/RT detected at Tmid = 1000
	Value computed using low-temperature polynomial:  19.8328
	Value computed using high-temperature polynomial: 19.9055


**** WARNING ****
For species SI2H6, discontinuity in s/R detected at Tmid = 1000
	Value computed using low-temperature polynomial:  49.5493
	Value computed using high-temperature polynomial: 49.7214


**** WARNING ****
For species SI3H8, discontinuity in h/RT detected at Tmid = 1000
	Value computed using low-temperature polynomial:  29.3028
	Value computed using high-temperature polynomial: 29.4297


**** WARNING ****
For species SI3H8, discontinuity in s/R detected at Tmid = 1000
	Value computed using low-temperature polynomial:  65.9731
	Value computed using high-temperature polynomial: 66.2781


**** WARNING ****
For species SI2, discontinuity in h/RT detected at Tmid = 1000
	Value computed using low-temperature polynomial:  74.0115
	Value computed using high-temperature polynomial: 74.0387


**** WARNING ****
For species SI2, discontinuity in s/R detected at Tmid = 1000
	Value computed using low-temperature polynomial:  32.8813
	Value computed using high-temperature polynomial: 32.9489
 
  silane:
 
       temperature            1500  K
          pressure             100  Pa
           density     1.83141e-05  kg/m^3
  mean mol. weight         2.28407  amu
 
                          1 kg            1 kmol
                       -----------      ------------
          enthalpy      1.7017e+07        3.887e+07     J
   internal energy      1.1557e+07         2.64e+07     J
           entropy      1.0387e+05        2.372e+05     J/K
    Gibbs function     -1.3878e+08        -3.17e+08     J
 heat capacity c_p           14162        3.235e+04     J/K
 heat capacity c_v           10522        2.403e+04     J/K
 
                           X                 Y          Chem. Pot. / RT    
                     -------------     ------------     ------------
                H2       0.995395         0.878516         -25.5277
                 H    0.000559189      0.000246765         -12.7639
                HE              0                0     
              SIH4    1.05394e-07      1.48198e-06         -50.9842
                SI     0.00105469        0.0129687        0.0713036
               SIH     1.2607e-05      0.000160581         -12.6926
              SIH2     1.1852e-05      0.000156195         -25.4564
              SIH3    1.18896e-07      1.61938e-06         -38.2203
           H3SISIH    6.98628e-12      1.84142e-10         -50.9129
             SI2H6    1.66065e-14      4.52364e-13         -76.4406
          H2SISIH2    1.78387e-10      4.70187e-09         -50.9129
             SI3H8    6.98199e-21      2.82205e-19         -101.897
               SI2    0.000120384       0.00296054         0.142607
               SI3     0.00284607         0.104988         0.213911

